**IPFusion Designer Training**

**Project Specification Worksheet**

|  |  |
| --- | --- |
| **Resources** | |
| Image 1 | Admin Background.png |
| Image 2 | Overview.png |
| Sound 1 | Notification.wav |

|  |  |
| --- | --- |
| **Screens** | |
| Screen 1 Caption | Site |
| Screen 1 Title | Site Overview |
| Screen 2 Caption | Network |
| Screen 2 Title | Network Maintenance |
| Screen Dimensions | 1185 x 500 |

|  |  |
| --- | --- |
| **Workstation 1** | |
| Name | WA |
| Description | Workstation A |
| Startup Screen | Site |

|  |  |
| --- | --- |
| **Workstation 2** | |
| Name | WB |
| Description | Workstation B |
| Startup Screen | Network |

|  |  |
| --- | --- |
| **Alarms** | |
| Alarm 1 | Default “Fault” |
| Alarm 2 | Default “No Communication” |
| Alarm 3 Name | Alarm |
| Alarm 3 Sound | Notification.wav |
| Alarm 3 Color | Red w/ Black Text |
| Alarm 3 Flash Color | White w/ Black Text |

|  |  |  |
| --- | --- | --- |
| **Milestone System** | | |
| Name | Milestone |
| Type | Milestone XProtect Corporate |
| Commands | Acknowledge, Reset, Clear |
| Data Server Address | 10.99.96.151 | |
| Data Server Port | 9030 | |
| Driver Server Address | 10.99.96.212 | |
| User Name | Operator | |
| Password | Operator | |
| Auth. Type | Windows | |
| Camera 1 Guid | 5F46F1DF-07A7-48EB-A61F-5C5397233F55 | |
| Camera 2 Guid | 44BCBC19-4613-4B4D-A2F6-D2B1BA601293 | |
| Camera 3 Guid | 89D54F03-1202-424B-B65F-305252E690AD | |
| Assets | Cameras C01, C02, C03 | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Harding System** | | | |
| Name | Harding | |
| Type | Harding DXL | |
| Commands | *Name* | *Function* |
|  | Acknowledge | Acknowledge |
|  | Reset | Reset |
|  | Call | Call |
|  | Clear | End Call |
| Data Server Address | 10.99.96.151 | | |
| Dataserver Port | 9522 | | |
| Master 1 ID | 82 | | |
| Master 1 Address | 10.1.100.233 | | |
| Master 1 Port | 10010 | | |
| Intercom IDs | 101, 102, 103 | | |
| Assets | Intercom I01, I02, I03 | | |

|  |  |  |
| --- | --- | --- |
| **Lenel System** | | |
| Name | OnGuard |
| Type | OnGuard |
| Commands | Enable Door, Disable Door (others are optional) |
| Data Server Address | 10.99.96.221 | |
| Data Server Port | 9002 | |
| Comm Settings | Yes – Driver is installed on server | |
| Door | Deivce1|Panel6, Device2|Panel6 | |
| Reader 1 | Panel6|Reader1 | |
| Reader 2 | Panel6|Reader2 | |
| Template Message Banner | ID, Timestamp, Details, Type | |

Add these entries to host file:

10.99.96.212 MilestoneWorkg1

10.99.96.153 MilestoneWorkg18b